System information "Minutes" time signal faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Time signal 'Minutes' within the CAN message 'Time/Date' faulty (CAN SPN 960). Effects on the driving operation Entries in the event memory contain no or faulty 'Time/Date identification'. Possible causes An incorrect value for 'Minutes' within the CAN message 'Time/Date' was received via the CAN bus (CAN SPN 960). Place of action No description available. Instruction Check CAN message 'Time/Date' on the CAN bus and make it available if necessary (if SAE J1939 CAN protocol is used). Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)