Gear enabling Faulty brake-switch signal via CAN SAE-J1939.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Faulty brake-switch signal via CAN SAE-J1939. Effects on the driving operation No gear enabling via the brake-switch signal via CAN SAE-J1939. No driving operation. Possible causes Gear enabling via the brake-switch signal via CAN SAE-J1939 is active and the brake-switch signal via the two CAN-messages CCVS and EBC1 is invalid or cannot be received. Place of action No description available. Instruction Check connector, cable the control units involved. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)