CAN Protocol SAE J1939 Timeout of message EBC1
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Timeout of the CAN receive message EBC1 (Electronic Brake Controller #1). Effects on the driving operation No retarder operation. Possible causes Brake / ABS controller defective or connection to brake / ABS controller faulted. Place of action No description available. Instruction Check brake / ABS controller or connection to brake / ABS controller. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)