TIM - Transmission Identification Module The TIM data in the TIM are inconsistent.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The TIM data in the TIM are inconsistent. Effects on the driving operation The transmission control unit cannot configure automatically anymore. (This also applies for a replacement control unit). This condition can lead to dangerous malfunctions when replacing the transmission control unit at the affected transmission! Driving is not possible. Possible causes Internal fault in the TIM. Place of action No description available. Instruction Reload the TIM data into the TIM. Replace TIM. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)