Analog-Digital Converter of E300 (ADC) ADC channel faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description ADC channel faulty. Effects on the driving operation No description available. Possible causes Faulty AD conversion of an ADC channel. (expert information: The value for an incorrect ADC channel was stored in the software’s ADC buffer. The cause is probably a timing problem in the software.) Place of action No description available. Instruction If problem reoccurs during regular operation, contact Voith and update software if necessary. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)