CAN Protocol SAE J1939 Incorrect byte number of message EC
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Incorrect byte number in the CAN receive message 'Engine Configuration'. Effects on the driving operation None. Possible causes Engine controller does not send the CAN message 'Engine Configuration' correctly according to SAE-J1939 standard. The CAN messages is too long. Fault in engine controller. Place of action No description available. Instruction No description available. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)