Monitoring of the safety computer (by the main computer) Incorrect solenoid valve voltages
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The safety computer does not recognize the solenoid valve voltages correctly. Effects on the driving operation Driving is not possible. Possible causes Defective solenoid valve plug connections. Defective solenoid valve wiring. Defective solenoid valve Internal fault of the safety computer Internal fault of the control unit Place of action No description available. Instruction Check plug connections and cables of the solenoid valves. Clear event memory If the fault cannot be eliminated, please contact the VOITH customer service. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)