Software module Event memory Buffer overflow in the event memory
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Troubleshooting
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Buffer overflow of the (reentrant-capable) event memory or requests of the (not reentrant-capable) event buffer outside time dials. The event memory can not save all events that apply simultaneously. Effects on the driving operation Event memory does not work correctly. Entries are lost. Possible causes Software system fault Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Instruction Load new software Send control unit file to VOITH customer service. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)