CAN gear range selector E330 The CAN gear selector switch has executed a wrong command.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The gear range selector has executed a different command than requested. The commands in the CAN send and receive messages are different. Effects on the driving operation Response depends on the command. Possible causes Defect in the CAN controller of the gear range selector or transmission controller. CAN communication disturbed, software fault in the gear range selector or in the transmission control unit. Place of action No description available. Instruction Check gear range selector and transmission control unit. Check whether the fault reoccurs. Replace the software of the transmission control unit. Contact Voith. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)