Monitoring of the safety computer (by the main computer) Transmission output speed (n2) not correct
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The safety computer does not detect the transmission output speed (n2) correctly. Effects on the driving operation Driving is not possible. Possible causes Defective n2 speed sensor plug connections. Defective n2 speed sensor wiring. Defective n2 speed sensor. Internal fault of the safety computer Internal fault of the control unit Place of action No description available. Instruction Check plug connections and cabling of speed sensor. Clear event memory If the fault can not be eliminated, please contact the VOITH customer service. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)