Engine load source PWM-signal (Bosch-EDC, MB-EMR, MB-FMR, VDO-EGas,...) Engine characteristic curve in dataset faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Fault in the engine curve in the data batch. Effects on the driving operation Hard, in strong engines no shifts. Possible causes Implausible values in the dataset constant ENG_TORQUE_CURVES_. Place of action No description available. Instruction Check/correct data batch constant ENG_TORQUE_CURVES_ prüfen/korrigieren. If this is not possible, replace the dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)