CAN-pushbutton switch E330 Buffer overflow while writing to the configuration memory (EEPROM)
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description A buffer overflow has occurred while writing to the configuration memory (EEPROM). Effects on the driving operation Modifications to the gear selector configuration were not applied (response depends on the modified data). Possible causes Too many simultaneous write jobs or waiting write jobs cannot be finished. Software problem. Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)