CAN 1 - Hardware Timeout in transmission control unit
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description At least one CAN message could not be sent within the timeout period of the send messages. Effects on the driving operation Vehicle does not drive or only with restrictions. Possible causes This error message is generated by the software and occurs when the control unit has problems sending. The CAN1 bus is offline or busy processing too many CAN messages. Place of action CAN bus Instruction Check utilisation of the CAN1 bus using appropriate tools. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)