CAN gear range selector E330 Fault monitoring the flexible output
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Connection of flexible output FLEXO-H1
|  | Connector pin assignment of CAN gear selector switch
|  | Place of action
|  | Troubleshooting
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description An error has been detected while monitoring the flexible output: The output has not switched on despite the activation signal or has not switched off despite the deactivation signal. However, no fault was recognized. Effects on the driving operation The flexible output at the gear range selector can be non-functional. Possible causes Flexible output of the gear range selector is defective / malfunctions. The CAN controller in the gear range selector or transmission control unit is defective / malfunctions. Connection of flexible output FLEXO-H1 Connector pin assignment of CAN gear selector switch
Pin | Name | Pin | Name | Pin | Name
1 | IGN | 6 | CAN-H | 11 | FLEXI-4
2 | -BATT | 7 | CAN-R | 12 | FLEXI-5
3 | CAN-L | 8 | FLEXI-1 | 13 | FLEXI-6
4 | CAN-L | 9 | FLEXI-2 | 14 | FLEXO-1H
5 | CAN-H | 10 | FLEXI-3 |  |
Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Check cabling of the flexible output. Check flexible output (activate and measure level, deactivate and measure level). If activation or deactivation does not work, the gear range selector should be replaced. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)