CAN gear range selector E330 The CAN gear selector switch was reconfigured.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The CAN gear range selector was reconfigured with the basic setting due to a fault. All existing settings have been deleted. The CAN gear range selector has been reconfigured with the basic settings due to a fault. All existing settings have been deleted. Effects on the driving operation All stored data are lost. The gear range selector starts in the basic setting: Consequences: Driving is not possible or restricted. the CAN bus is overloaded. The fabrication data have been deleted. Flexible output and flexible inputs could be non-functional. Possible causes Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)