Operating data The internal operating data structure was destroyed in such a way that an external evaluation was impossible.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description The internal operating data structure was destroyed in such a way that an external evaluation was impossible. The operating data structure was reorganized. Effects on the driving operation No system response. Possible causes FRAM error (memory error), faulty pointer accesses, version conflicts, software errors,... Location No location. Instruction No further actions required. Self-healing has been carried out. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)