TIM - Transmission Identification Module The TIM data in the TIM are inconsistent.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Connector pin assignment of the transmission control unit
|  | Connector pin assignment of the transmission connector
|  | Internal cable harness
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The TIM data in the TIM are inconsistent. Effects on the driving operation The transmission control units (other transmission control units too!) can no longer configure themselves automatically. This condition can lead to dangerous malfunctions when replacing the transmission control unit at the affected transmission! The vehicle can no longer be moved. Possible causes Internal fault in the TIM. Connector pin assignment of the transmission control unit
Pin | Stecker A | Stecker B | Stecker C | Stecker D
1 | SHIELD | EK | FLEXI-1 | -BATT
2 | TIM+ | DK | --- | IGN
3 | TIM- | SK | FLEXI-3 | FLEXI-11
4 | N1+ | RBK | FLEXI-4 | K-LINE
5 | N1- | TB | FLEXI-5 | CAN1-H
6 | N2+ | --- | FLEXI-6 | CAN1-H
7 | N2- | RBG | FLEXI-7 | CAN-SHLD
8 | N3+ | PB | FLEXI-8 | CAN1-L
9 | N3- | WR | FLEXI-9 | CAN1-L
10 | --- | WP | FLEXI-10 | CAN2-H
11 | --- | --- | FLEXO-2H | CAN2-H
12 | EKM | FLEXI-12 | FLEXO-4H | CAN2-L
13 | DKM | S-GND | FLEXO-3H | CAN2-L
14 | SKM | OIL-LVL | FLEXO-5L | CAN1-R
15 | PBM | T-SUMP | --- | ---
16 | TBM | --- | --- | FLEXO-1L
17 | RBKM | T-CONV | --- | CAN2-R
18 | MVM-GND | MV-GND | --- | +BATT
Connector pin assignment of the transmission connector
Pin | Name | Pin | Name | Pin | Name
1 | S-GND | 14 | RBK | 27 | EKM
2 | MV-GND | 15 | RBG | 28 | PBM
3 | MV-GND | 16 | TB | 29 | RBKM
4 | --- | 17 | WR | 30 | TBM
5 | T-CONV | 18 | --- | 31 | MVM-GND
6 | T-SUMP | 19 | --- | 32 | N1+
7 | OIL-LVL | 20 | --- | 33 | N1-
8 | P-DIFF | 21 | TIM- | 34 | N2+
9 | SK | 22 | TIM+ | 35 | N2-
10 | DK | 23 | --- | 36 | N3+
11 | EK | 24 | SHIELD | 37 | N3-
12 | PB | 25 | SKM |  |
13 | WP | 26 | DKM |  |
Internal cable harness Place of action Data in the TIM. Instruction Reload the TIM data into the TIM. Replace TIM. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)