CAN Protocol SAE J1939 Timeout of message TSC1 from system 3
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Timeout of the CAN receive message TSC1 (Torque/Speed Control #1) of system 3. Effects on the driving operation Retarder function requested via this message not available. Possible causes Controller for retarder setpoint setting or connection to this controller is faulted. Place of action No description available. Instruction Check controller for retarder setpoint setting and connection to this controller. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)