CAN protocol SAE J1939 Timeout of message TD
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Troubleshooting
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Timeout of the CAN receive message TD (Time/Date). Effects on the driving operation If faults occur in the transmission control unit, it may not be possible to store date and time as additional information to the fault in the event memory. Possible causes Controller for vehicle control or connection to this controller is faulted. Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Check controller for vehicle control and connection to this controller. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | CAN SAE J1939 Voith specifics (SW E300-D2.3.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300-D2.4.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300.1-D5.0.0.0)
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)