TIM - Transmission Identification Module Invalid parameters in the command
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The TIM command manager has received invalid parameters while initiating a command. Effects on the driving operation No communication with the TIM possible. Unable to read the transmission-specific data. The vehicle might drive with the wrong transmission configuration. Possible causes The software version of the transmission control unit does not match the software version of the TIM. Internal fault in the transmission control unit. Internal fault in the TIM. Place of action ECU software, TIM. Instruction Reload software in the transmission control unit. Clear the fault memory . If the fault reoccurs, contact the Voith customer service. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)