TIM - Transmission Identification Module Transmission data: Input torque is wrong.
|  | Final function check
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly. Description Transmission data: Input torque is wrong. Effects on the driving operation The transmission-specific data is wrong. The vehicle might drive with the wrong transmission configuration. The newly specified transmission configuration was not accepted. Possible causes The newly specified input torque is wrong. Location Screen form/input interface. Instruction The input torque must correspond to an actually existing torque specification. Setting conditions for the event No description available. Test conditions for the event No description available.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)