Brake switch signal source hand brake switch 3-stage Short-circuit or low-resistance connection to supply voltage at brake switch input 2.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
|  | See also:
Description Short-circuit or low-resistance connection to supply voltage at brake switch input 2. Effects on the driving operation No description available. Possible causes Short-circuit in cable, connector or brake switch. Place of action No description available. Instruction Check plug connections, cabling and brake switch, if applicable. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly. See also:
|  | Troubleshooting for short-circuit to 24 V
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)