CAN Protocol VOITH private CAN Timeout of message INPUT VALUES 0
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Timeout of CAN message INPUT VALUES 0. Effects on the driving operation Functions using the flexible inputs of the gear range selector are not available. Possible causes Connection to gear range selector faulted or gear range selector defective. Incorrect voltage supply of the gear range selector. Place of action No description available. Instruction Check connection to the gear range selector and the gear range selector. Check voltage supply of the gear range selector. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)