Gear enabling No SAE-J1939 protocol during gear enabling via the brake-switch signal via CAN SAE-J1939.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description No SAE-J1939 protocol during gear enabling via the brake-switch signal via CAN SAE-J1939. Effects on the driving operation No gear enabling. No driving operation. Possible causes Gear enabling via the brake-switch signal via CAN SAE-J1939 is active and no SAE-J1939 protocol was set in the dataset for the value CAN_PROTOKOLL_PUBLIC_CAN_. Place of action No description available. Instruction Request new dataset from Voith. Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)