Gear enabling Brake pedal position for gear enabling is set too small in the dataset.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Brake pedal position for gear enabling is set too small in the dataset. Effects on the driving operation No gear enabling. No driving operation. Possible causes Gear enabling with the brake pedal position is active and GEAR_ENBL_BRAKE_PEDAL_POS_MIN_ was set smaller than 5% in the dataset. Place of action No description available. Instruction Request new dataset from Voith. Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)