Transmission detection Unknown fault.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | See also:
Description Unknown fault. Effects on the driving operation Hard shifts Driving in reverse gear is not possible or restricted. If the output sensor is also defective, only limp-home mode available No torque limitation relative to the engine speed Engine torque reduction is limited. The characteristic curve of the auxiliaries is not considered. The engine speed and values derived from it are incorrectly set in the CAN communication. Possible causes An unknown fault has occurred. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Check plug connections, cabling and sensor. Setting conditions for the event No description available. Test conditions for the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)