CAN Protocol VOITH private CAN Timeout of message TC1
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Timeout of message TC1 (Transmission Control 1). Effects on the driving operation Driving is not possible. Possible causes Communication to the gear selector is disturbed or gear selector defective. Incorrect voltage supply of the gear range selector. Place of action No description available. Instruction Check communication to the gear selector and the gear selector itself. Check voltage supply of the gear range selector. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | CAN SAE J1939 Voith specifics (SW E300-D2.3.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300-D2.4.0.0)
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)