Engine speed sensor Sensor voltage too high
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Sensor voltage too high If the sensor voltage exceeds 14 V, the speed sensor signal cannot be evaluated anymore. Effects on the driving operation Hard shifts. No switching into reverse gear. Main pressure to maximum. Reduction of the engine torque to protect the transmission. If the engine transmission output speed sensor is simultaneously defective, only limp-home mode available. The engine speed and/or the values derived on its basis are incorrectly set in the CAN communication. Possible causes Low-resistance connection of the positive sensor terminal to supply voltage or defect of the transmission control unit Place of action Engine speed sensor (sensor voltage) Instruction Measure voltage at the speed sensor. Check plug connections, cabling and sensor. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)