Control unit connector / transmission connector Control unit connectors A and B at the E300.1 control unit and/or transmission connector are disconnected
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Connector pin assignment of the transmission control unit
|  | Connector pin assignment of the transmission connector
|  | Internal cable harness
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description The control unit connectors A and B at the E300.1 control unit and/or the transmission connector are disconnected. Effects on the driving operation No driving operation possible. Possible causes Connector disconnected (at least 3 of the connected actuators/sensors signal line interruption). Connector pin assignment of the transmission control unit
Pin | Stecker A | Stecker B | Stecker C | Stecker D
1 | SHIELD | EK | FLEXI-1 | -BATT
2 | TIM+ | DK | --- | IGN
3 | TIM- | SK | FLEXI-3 | FLEXI-11
4 | N1+ | RBK | FLEXI-4 | K-LINE
5 | N1- | TB | FLEXI-5 | CAN1-H
6 | N2+ | --- | FLEXI-6 | CAN1-H
7 | N2- | RBG | FLEXI-7 | CAN-SHLD
8 | N3+ | PB | FLEXI-8 | CAN1-L
9 | N3- | WR | FLEXI-9 | CAN1-L
10 | --- | WP | FLEXI-10 | CAN2-H
11 | --- | --- | FLEXO-2H | CAN2-H
12 | EKM | FLEXI-12 | FLEXO-4H | CAN2-L
13 | DKM | S-GND | FLEXO-3H | CAN2-L
14 | SKM | OIL-LVL | FLEXO-5L | CAN1-R
15 | PBM | T-SUMP | --- | ---
16 | TBM | --- | --- | FLEXO-1L
17 | RBKM | T-CONV | --- | CAN2-R
18 | MVM-GND | MV-GND | --- | +BATT
Connector pin assignment of the transmission connector
Pin | Name | Pin | Name | Pin | Name
1 | S-GND | 14 | RBK | 27 | EKM
2 | MV-GND | 15 | RBG | 28 | PBM
3 | MV-GND | 16 | TB | 29 | RBKM
4 | --- | 17 | WR | 30 | TBM
5 | T-CONV | 18 | --- | 31 | MVM-GND
6 | T-SUMP | 19 | --- | 32 | N1+
7 | OIL-LVL | 20 | --- | 33 | N1-
8 | P-DIFF | 21 | TIM- | 34 | N2+
9 | SK | 22 | TIM+ | 35 | N2-
10 | DK | 23 | --- | 36 | N3+
11 | EK | 24 | SHIELD | 37 | N3-
12 | PB | 25 | SKM |  |
13 | WP | 26 | DKM |  |
Internal cable harness Location Control unit connector A, B and/or transmission connector. Instruction Connect the plug connections to the control unit and/or the transmission. Check for tight fitting. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)