Safety computer CAN-bus off
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description A CAN bus off was detected. The CAN controller has detected that there are no other bus parties on the CAN bus. Effects on the driving operation Driving is not possible or restricted. Possible causes The control unit has no connection to the other bus parties. Place of action No description available. Instruction Check terminating resistors. Check CAN bus including all bus parties. Clear event memory Should the fault reoccur, please contact the VOITH customer service. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)