ABS input signal Datensatzfehler in Signalzuordnung zu einem Ausgang
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Dataset fault in the signal assignment to an input of the E300. Effects on the driving operation No retarder operation. No ANS-function Possible causes The assignment of the digital ABS-signal to an input of the E300 via the dataset is faulty. Place of action No description available. Instruction Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)