ABS input signal ABS via digital input permanently active
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description ABS via digital input permanently active. Effects on the driving operation No retarder operation No ANS-function Possible causes Faulty connection of the ABS connector pin to ground or cable break or defective external ABS-controller. In vehicles without ABS the ABS connector pin must be connected to operating voltage. Place of action No description available. Instruction Check connector/cable. Check the external ABS-controller. In vehicles without ABS the ABS connector pin must be connected to the operating voltage or the dataset value FLEXI_ABS_SETTING_ must be set to 0. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)