CAN Protocol SAE J1939 Timeout of message TC1
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Timeout of receive message TC1 (Transmission Control 1). Effects on the driving operation Driving only possible via LIMP-HOME switch. Possible causes Controller for direction setting (gear range selector / on-board computer) or connection to this controller is faulted. Place of action No description available. Instruction Check for the VOITH gear range selector whether the lamp test is carried out (i.e. voltage supply is o.k.). If all start to flash after 10 seconds, the CAN connection to the transmission controller is interrupted. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)