Gear enabling The digital input for gear enabling provides a faulty signal.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The digital input for gear enabling provides a faulty signal. Effects on the driving operation No gear enabling via digital input. No driving operation. Possible causes Gear enabling via a digital input is active and the value FLEXI_GEAR_ENBL_SETTING_ was set to an implausible value in the dataset. Place of action No description available. Instruction Request new dataset from Voith. Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)