Output signal SPD-SIG ( speed signal ) Fault in the data batch constant FLEXO_SPD_SIG_SETTING_
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Fault in the data batch constant FLEXO_SPD_SIG_SETTING_. Effects on the driving operation The output signal can no longer change in relation to the output speed. The signal is evaluated by external control units, e.g. the door control may be affected. Possible causes The data batch value FLEXO_SPD_SIG_SETTING_ contains a faulty or invalid value. Place of action No description available. Instruction Correct data batch value FLEXO_SPD_SIG_SETTING_ or load the correct data batch. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)