Engine speed sensor Implausible frequency
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Implausible frequency Effects on the driving operation Hard shifts. No switching into reverse gear. Main pressure to maximum. Reduction of the engine torque to protect the transmission. If the engine transmission output speed sensor is simultaneously defective, only limp-home mode available. The engine speed and/or the values derived on its basis are incorrectly set in the CAN communication. Possible causes Implausible speed ratios between engine output speed and transmission output speed have been measured in the mechanical gear which are not possible due to the transmission ratio. Attention: The output speed sensor can also be the cause of this fault! Possible causes: The sensors are installed in the wrong position, defect of the speed sensors, no correct adhesion of the disks. Place of action Transmission mechanics Engine speed sensor Transmission output speed sensor Instruction Check all frequency transmitters for correct signal generation and correct installation (check the distance to the measurement gear). Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)