Brake switch signal source hand brake switch 3-stage Brake switch input 2 inadmissibly active
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Brake signal input 2 inadmissibly active Effects on the driving operation No retarder activation Possible causes Implausible brake switch signals have occurred which indicate that the input is permanently active. The following causes are possible: * Short-circuit to the 'active side' of the input signals. (The 'active side' is derived from the content of the dataset constant that is relevant for the signal configuration). ) Place of action No description available. Instruction Check plug-in contacts, cabling and brake switch. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)