CAN-pushbutton switch E330 Basic settings due to a fault are reconfigured.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The CAN-pushbutton was reconfigured with the basic setting due to a fault. All existing setting have been deleted. The CAN-pushbutton was reconfigured with the basic setting due to a fault. All existing settings have been deleted. Effects on the driving operation All set data get lost. The gear range selector starts in the basic setting: Driving is not possible or restricted. The CAN bus is overloaded. The fabrication data have been deleted. Flexible output and flexible inputs could be non-functional. Possible causes Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)