Transmission oil temperature sensor E300 Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | See also:
Description Undiagnosible fault Effects on the driving operation Unable to detect temperature, possible consequences: Hard shifts with transmission oil cold. The temperature-related deactivation of the retarder is restricted. Possible causes The cause could be a cable break or short-circuit to supply voltage. If the error 'Reference voltage too high' is also present, this indicates a short-circuit to supply voltage. If only one temperature sensor reports this fault, there is probably a cable break at this sensor. Place of action No description available. Instruction Check plug connections, cabling and sensor. Setting conditions of the event No description available. Test conditions of the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)