ABS input signal ABS-signals via CAN implausible
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Connection of the ABS
|  | Connector pin assignment of transmission control unit
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Troubleshooting
|  | Final function check
|  | See also:
Description ABS signals via CAN implausible. Effects on the driving operation No retarder operation No ANS-function Possible causes The ABS-CAN signals sent on the CAN bus are contradictory. Using the SAE J1939 CAN protocol: EBC1 (Electronic Brake Controller #1) CAN message: The CAN signals ´ABS active´ and ´ABS fully operational´ must have both values unequal 0xFFFF. This fault occurs if one of the two CAN signals has the value 0xFFFF and the other signal a valid value or a fault id. Connection of the ABS Connector pin assignment of transmission control unit
Pin | Stecker A | Stecker B | Stecker C | Stecker D
1 | SHIELD | EK | FLEXI-1 | -BATT
2 | TIM+ | DK | --- | IGN
3 | TIM- | SK | FLEXI-3 | FLEXI-11
4 | N1+ | RBK | FLEXI-4 | K-LINE
5 | N1- | TB | FLEXI-5 | CAN1-H
6 | N2+ | --- | FLEXI-6 | CAN1-H
7 | N2- | RBG | FLEXI-7 | CAN-SHLD
8 | N3+ | PB | FLEXI-8 | CAN1-L
9 | N3- | WR | FLEXI-9 | CAN1-L
10 | --- | WP | FLEXI-10 | CAN2-H
11 | --- | --- | FLEXO-2H | CAN2-H
12 | EKM | FLEXI-12 | FLEXO-4H | CAN2-L
13 | DKM | S-GND | FLEXO-3H | CAN2-L
14 | SKM | OIL-LVL | FLEXO-5L | CAN1-R
15 | PBM | T-SUMP | --- | ---
16 | TBM | --- | --- | FLEXO-1L
17 | RBKM | T-CONV | --- | CAN2-R
18 | MVM-GND | MV-GND | --- | +BATT
Place of action No description available. Instruction Check cable and connector of the CAN connection. Check the external ABS-controller. Using the CAN-SAE-J1939-protocol: EBC1(Electronic brake controller #1) -Verify CAN-message Setting conditions of the event No description available. Test conditions of the event No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | CAN SAE J1939 Voith specifics (SW E300-D2.3.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300-D2.4.0.0)
|  | CAN SAE J1939 Voith specifics (SW E300.1-D5.0.0.0)
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)