Engine torque reduction Allowed engine torque exceeded while shifting gears
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description Allowed engine torque exceeded while shifting gears Effects on the driving operation Transmission overload while shifting. Possible causes 1. The engine does not respond to the engine specification from the transmission control unit. 2. The transmission control unit sends incorrect torque specifications. Place of action No description available. Instruction Check the specified torque from the transmission control unit an make sure that the engine responds correctly to the requested reduced torque. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)