CAN-pushbutton switch E330 Faulty neutral-not signal
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description A fault has been detected while monitoring the neutral-not signal: The neutral-not signal is active for too long without a button applied Effects on the driving operation No limitations. Possible causes Feuchtigkeit in Tastenschalter eingedrungen. Gear range selector defective. Place of action No description available. Instruction Clear fault and apply neutral at the gear selector and wait approx. 5 seconds. If the fault is re-entered, replace the gear range selector! Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)