Safety computer The safety computer has detected the status "waiting for neutral" in the driving mode.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The safety computer has detected the "Waiting for neutral" state. Effects on the driving operation The solenoid valves can not be activated until this condition has been eliminated. If the conditions has been eliminated, it is necessary to engage neutral first before another gear request is accepted. Possible causes The signal for the gear request is not stable. The voltage of the electric system is unstable. Place of action No description available. Instruction Check the signal for the gear request. Check voltage of the vehicle’s electric system. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)