CAN Protocol IES Invalid CAN controller number in dataset
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Invalid CAN controller number in dataset. Effects on the driving operation All input signals of the IES protocol are not available. IES protocol messages are not sent. Possible causes Faulty value in the dataset variable CAN_CONTROLLER_NUMBER_PUBLIC_CAN_. Place of action No description available. Instruction Change the dataset value CAN_CONTROLLER_NUMBER_PUBLIC_CAN_ or load a suitable dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)