Brake signal source 3-stage foot brake pedal The dataset value FLEXI_FB1_SETTING_G_ for brake switch input 1 is faulty.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The dataset value FLEXI_FB1_SETTING_ for brake switch input 1 is faulty. Effects on the driving operation The ECU switches into the mode "forced neutral". Driving is not possible. Possible causes The signal of the input is not configured correctly in the dataset. Place of action No description available. Instruction Check the dataset; correct it or load an updated dataset. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)