Software module Identification Data Invalid identifier: hardware serial number
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Invalid identifier: hardware serial number. Effects on the driving operation No description available. Possible causes The hardware serial number read out of the manufacturer area is not valid. The value was either overwritten or incorrectly entered. Valid values are between 1...999999. The (transmission) function software has entered the default value "1". Place of action No description available. Instruction Replace control unit Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)