Brake switch signal source for service foot brake switch 3-stage Data batch value FLEXI_FB3_SETTIN_G_ for the brake switch input 3 faulty.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Data batch value FLEXI_FB3_SETTING_ for the brake switch input 3 faulty. Effects on the driving operation Operation mode forced neutral. No driving operation. Possible causes The signal of the input is not configured correctly in the dataset. Place of action No description available. Instruction Correct data batch value FLEXI_FB3_SETTING_ or load the correct data batch. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)