ABS input signal ABS via CAN permanently active
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description ABS via CAN permanently active Effects on the driving operation No retarder operation No ANS-function Possible causes External control unit sends a permanently active ABS through the CAN bus by the CAN signal "ABS active". Place of action No description available. Instruction Check the external ABS-controller. Using the CAN-SAE-J1939-protocol: EBC1(Electronic brake controller #1) -Verify CAN-message Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)