ANS (Automatic Neutral at Standstill) Malfunction of the feedback concerning the activated roll-away protection
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
Description Malfunction of the feedback concerning the activated roll-away protection Effects on the driving operation No ANS function Possible causes The activation of the roll-away protection on request of the transmission control has not been confirmed by the vehicle. The activation of the roll-away protection has been confirmed by the vehicle though there is no request by the transmission control. The confirmation concerning the activation of the roll-away protection has been cancelled though the request by the transmission control still existed. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Check the vehicle cabling. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)