Engine load signals via CAN CAN signal for engine torque setpoint faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
|  | See also:
Description CAN signal for engine torque setpoint faulty. Effects on the driving operation No acceleration limitation possible. Possible causes A CAN message required to determine the current engine torque setpoint provides (a) faulty value(s). Using the SAE J1939 CAN protocol: CAN message 'EEC1' : 'drivers demand engine-percent torque' faulty. For information on the affected CAN message, please refer to the system description. Location No description available. Instruction Check the CAN message / CAN signal and correct if necessary. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)